**\_10\_ -** Changelog:

1. Changed allowed lag range to 2-22 ms (was previously 4-12 ms). This is based on King et al., 2016, who used 0-20 ms after subtracting out tube delay (we did not subtract out tube delay, so nudged by 2 ms).

**\_9\_** - Changelog from \_8\_:

* Fixed a bug where FFR was getting windowed at 40 *samples* instead of 40 *milliseconds* worth of samples (800 samples). Also
* Fixed a bug that sometimes caused the function to crash when parsing the output directory.
* Fixed a bug that caused this function to erase saved data in the MAT file from the xcorrByWin function.

All other versions are obsolete.